1. M3 hex nut for bottom plate
2. M3 12mm machine screws
3. Print with 1.1 extrusion multiplier and 220C nozzle temp for all layers. 0.2mm layers.
4. PLA filament